
**How to Disable SIP ALG on TP-Link ADSL modem router**

**Suitable for:** TD-8816, TD-8817, TD-8840T, TD-8841T, TD-W8101G, TD-W8901G

For the VOIP application, sometimes the ISP will ask you to disable SIP ALG on your modem router. Please refer to the following steps to do the configuration.


**Step 1**Press the **Windows Logo Keyhttp://uk.tp-link.com/resources/images/faq/2011689264387.jpg**+"**R**" Key on the Keyboard at the same time or click on **Start button**->**Run** to open Run program.

**Step 2**Type in **cmd** in the open bar and click **OK**.




**NOTE:**In **Windows 7**,you can also just type **cmd** in the search bar and

press **Enter** instead of above two steps .




**Step 3** Type in "**telnet** **192.168.1.1**" (192.168.1.1 is the default IP Address of the modem router, if you have changed it, please type in the matched IP) and press **Enter**.



**NOTE:**In Win7 or Vista, the telnet command may not be enabled by default, please click on**Start button**->**Control Panel**->**Programs**-> **Programs And Features**->**Turn Windows features on or off**,then Check **Telnet Client** and hit OK to enable telnet command.

**Step 4** In the telnet page, type in the password for the modem router (default is **admin**) and press **Enter**.

**Step 5** Type in command **ip nat service sip sw off**.If SIP ALG is disabled successfully, it will show **Nat Sip v2 switch off!**

****

**NOTE：**

All of the above settings are temporary. Once you **restart** or **reset** the modem, the SIP ALG will be turned back on.